|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Common settings DMR / FM:** | | | |  | | | | | |
|  |  | | | | | | | | |
| RF Power | [Fn] + [▲] or [Fn] + [▼] | | | | | | | | |
| Channel details | [Sk1] | | | | | | | | |
| Reverse mode | long press [**#**] | | | | | | | | |
| DMR or FM selection | [Fn] + [🞳] | | | | | | | | |
|  |  | | | | | | | | |
|  |  | | | | | | | | |
| Freq. / channel select | [select] knob | | | | | | | | |
| VFO or Memory mode |  | | | | | | | | |
| Memory mode:  channel selection | turn [select] knob | | | | | | | | |
| VFO mode: VFO A or B | long press | | C:\Users\wkm\AppData\Local\Microsoft\Windows\INetCache\Content.Word\78ObPhbMyN_Radiant -s.jpg | | |  | | | |
| VFO mode: Tx or Rx selection | [Fn] + [select] | | | | | | | | |
| VFO mode: Freq. entry | num keys, store with | | | | C:\Users\wkm\AppData\Local\Microsoft\Windows\INetCache\Content.Word\BULfXGQ69V_Radiant green s.jpg | |  | |  |
| Scanning ON | long press [▲] | | | | | | | | |
| Scanning OFF | any num key or rotate [selct] ⭯ | | | | | | | | |
|  |  | | | | | | | | |
| **FM mode:** |  | | | | | | | | |
|  |  | | | | | | | | |
| Squelch setting | Short press [▲] or [▼] | | | | | | | | |
| Open squelch | [Fn] | | | | | | | | |
| Send 1750 Ht tone | [Fn] + [PTT] | | | | | | | | |
|  |  | | | | | | | | |
| **Other functions:** |  | | | | | | | | |
|  |  | | | | | | | | |
| [PTT] lock ( disable [PTT] ) | C:\Users\wkm\AppData\Local\Microsoft\Windows\INetCache\Content.Word\BULfXGQ69V_Radiant green s.jpg | followed by [**#**] | | | |  | |  | |
| Keybooard lock | C:\Users\wkm\AppData\Local\Microsoft\Windows\INetCache\Content.Word\BULfXGQ69V_Radiant green s.jpg | followed by [🞳] | | | |  | |  | |
|  |  | | | | | | | | |
| Firmware load mode | Power OFF – hold [Fn] + [PTT] – power ON | | | | | | | | |
|  | LED should blink red / green | | | | | | | | |

|  |  |  |  |
| --- | --- | --- | --- |
| **DMR settings:** |  | | |
|  |  | | |
| TG list, selection | [▲] or [▼] | | |
| TG, manual input | [**#]** + enter TG num., followed by | C:\Users\wkm\AppData\Local\Microsoft\Windows\INetCache\Content.Word\BULfXGQ69V_Radiant green s.jpg | |
| Private call, accept | C:\Users\wkm\AppData\Local\Microsoft\Windows\INetCache\Content.Word\BULfXGQ69V_Radiant green s.jpg |  | |
| Private call | [**#**] [**#**] enter ID num., followed by | C:\Users\wkm\AppData\Local\Microsoft\Windows\INetCache\Content.Word\BULfXGQ69V_Radiant green s.jpg | |
| Contact | [**#**] [**#**] [**#**], than select with  [▲] or [▼], followed by | C:\Users\wkm\AppData\Local\Microsoft\Windows\INetCache\Content.Word\BULfXGQ69V_Radiant green s.jpg | |
| Remark: | Entries [**#**] [**#**] or [**#**] [**#**] [**#**] must be pressed in fast sequence. | |  |